* steering cards
> Lcalib                    , calibration run?
.FALSE.
> Lcalhist                  , calibration histograms for each group?
.FALSE.
> LDData                    , write Dense Data?
.FALSE.
> LPRF                      , use PadResponeFunction?
.TRUE. 
> Lplot                     , enable event plots?
.TRUE.  
*
* Thresholds
> minSignal                 , min level for a signal     
1.0
*3.0 
> smallSignal               , min level to determine T0 from this pulse (don't recalc with common T0)
5.0  
> minSignalVeto             , min level in Veto couter to reject event
5.0  
> minSignalRow              , min level of signal in a row
8.5  
> minSignalCalib            , min level of signal used for calibration
10.0 
> minDistPad                , min distance between pads to be called adjacent  
0.1  
> minHitTrack               , min number of rows with signal > minSignalRow requied for a track
 16
*12    
*
* pulse shape and fitting stuff
> driftVelocity               , timebin(DD=0), ns/timebin, vDrift (cm/ns)
 0.  40.   7.65E-3                     
> trackWidth                , coefficients for track width**2 vs driftdistance (cm): s**2 = p0 + DD*p1 + DD**2*p2 + ... :  p0 ~ padWidth**2 blindly
 21.2
> PRFdel                    , coefficients for del = p0 + DD*p1 + DD**2*p2 + ... , PadResponseFunction basewidth : p0 ~ 3.5 * padWidth
 11.3
> PRFa                      , PadResponseFunction parameter  a
 0.6
> PRFb                      , PadResponseFunction parameter  b
 0.
> AERRpar                   , amplitude error for chisq fit  (see code!!)
 3.
> FitType                   , type of track fit: 1=likelihood ; 2=likelihood truncated ; 3=chisq
 3
* 
* Scale factor / gain for fitting
*
* Tshift is also used as time window in T0 fit, must be >~10
> Tshift                    , difference between TMax and T0
20
* 
