Homework problems for normal conducting rf

Section 1

1.1 Imagine that the waveguide standard WR-97 existed. Plot the dispersion curve. What is the cutoff frequency? What are the group and phase velocities at 1.2, 1.5, 2 and 10 times this frequency?

1.2 What is the transit time factor for a cavity operating at 11.994 GHz which is one third of a wavelength long? At which phase should you inject to get maximum acceleration? To get zero acceleration? At which length would such a cavity not give any acceleration?

1.3 Plot the following disk loaded waveguide dispersion curves along with the phase and group velocity.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6 mm |  |  | 3 mm |  |
| 0 | 10530194428 |  | 0 | 11789563652 |
| 10 | 10544884522 |  | 10 | 11791704341 |
| 20 | 10588438665 |  | 20 | 11798147902 |
| 30 | 10659540055 |  | 30 | 11808517016 |
| 40 | 10756048590 |  | 40 | 11822597481 |
| 50 | 10874671328 |  | 50 | 11839943852 |
| 60 | 11012127448 |  | 60 | 11860049565 |
| 70 | 11163734072 |  | 70 | 11882251163 |
| 80 | 11325437241 |  | 80 | 11905853130 |
| 90 | 11492412104 |  | 90 | 11930207198 |
| 100 | 11658954444 |  | 100 | 11954538315 |
| 110 | 11820739142 |  | 110 | 11978108377 |
| 120 | 11972028973 |  | 120 | 12000204306 |
| 130 | 12109341843 |  | 130 | 12020159331 |
| 140 | 12228070989 |  | 140 | 12037372687 |
| 150 | 12324701847 |  | 150 | 12051327206 |
| 160 | 12396260365 |  | 160 | 12062294745 |
| 170 | 12440130247 |  | 170 | 12068960981 |
| 180 | 12454846032 |  | 180 | 12070540024 |

Section 2

2.1 An 11.994 GHz cavity 8.332 mm long has an R/Q=139 kohm/m. A 1 nC charge traverses the cavity. How much energy is deposited in the fundamental mode? What accelerating gradient does this correspond to?

2.2 The middle cell of a CLIC accelerating structure has 2pi/3 phase advance, a Q of 6200, a shunt impedance of 100 Mohm/m and a group velocity vg/c=1%. What is the accelerating gradient in the cell for a power flow of 50 MW? What is the stored energy per meter and per cell?

2.3 Assume that a travelling wave accelerating structure is built out of 30 of such cells. What is the accelerating gradient as a function of distance for an input power of 50 MW? What is the average accelerating gradient over the whole structure? What is the output power from the structure?

2.4 What current is required to obtain full beam loading in the structure? Plot the gradient along the structure. What is the total voltage of the structure? What would be the rf to beam efficiency for that current? Do the analysis again for half that current. What do you conclude?

2.5 Let’s keep driving this structure with the I/2 current but make the structure longer and longer and longer. What happens?

Section 5

5.1 A structure has a dipole mode frequency equal to 18 GHz with amplitude 1. Plot the long range wake. How could you make a structure one half has a dipole wake of 18 GHz and the other half has a dipole wake of 19 GHz? What would the long range wake be? Where would you put a second bunch in a train? What about the third? How would it change if you doubled the bandwidth (ie half at 18 GHz and the other at 20 GHz)? Now let’s go back to 1 GHz bandwidth. What happens to the wake if you make the structure out of 4 and 8 geometries? Compare the detuned-wake to the damped cell with a Q of 20. What differences do you see and why? Where would you put following bunches? Restricting yourself to 1 GHz bandwidth and 16 frequencies, mess around with something and try to improve the wake in different ways.

Section 6

6.1 The following two set of current vs. voltage data were taken in the CERN dc spark set-up. What was the field enhancement factor β and the emission area in each case.

Case 1 Gap distance 29.7 microns Case 2 Gap distance 18.8 microns

|  |  |  |  |
| --- | --- | --- | --- |
| **Voltage V [V]** | **Current I [A]** | **Voltage V [V]** | **Current I [A]** |
| 3100 | 1.22E-11 | 600 | 1.53E-11 |
| 3150 | 1.66E-11 | 625 | 5.07E-11 |
| 3200 | 2.07E-11 | 650 | 1.47E-10 |
| 3250 | 2.68E-11 | 675 | 3.96E-10 |
| 3300 | 2.84E-11 | 700 | 8.57E-10 |
| 3350 | 3.83E-11 | 725 | 1.69E-09 |
| 3400 | 5.04E-11 | 749 | 3.42E-09 |
| 3450 | 5.77E-11 | 774 | 5.60E-09 |
| 3500 | 6.78E-11 |  |  |
| 3550 | 8.65E-11 |  |  |
| 3600 | 1.03E-10 |  |  |
| 3650 | 1.19E-10 |  |  |
| 3700 | 1.38E-10 |  |  |
| 3750 | 1.28E-10 |  |  |
| 3800 | 1.50E-10 |  |  |
| 3850 | 2.12E-10 |  |  |
| 3900 | 2.46E-10 |  |  |
| 3950 | 2.79E-10 |  |  |
| 4000 | 3.21E-10 |  |  |
| 4050 | 3.80E-10 |  |  |
| 4100 | 4.53E-10 |  |  |
| 4150 | 5.14E-10 |  |  |
| 4200 | 5.90E-10 |  |  |
| 4250 | 7.00E-10 |  |  |
| 4300 | 8.59E-10 |  |  |
| 4350 | 1.06E-09 |  |  |